“世纪梦想”豪华游轮装饰工程项目

**船员家具手册**

【船员家具】

重庆冠达世纪游轮有限公司



**船员家具技术说明**

**Crew Furniture Technology Explain**

1.产品制造商（销售商）承诺产品质量符合国家标准和行业标准，以及相关规范要求。

1.The product manufacturer (seller) promises that the product quality meets national and industry standards, as well as relevant regulatory requirements.

2.材料采用多层实木免漆板，根据家具用料部位的不同而采用9mm-25mm不等的厚度，具体以世纪游轮确认图纸为准。材料环保等级必须达到E1级及以上。

2.The material used is multi-layer solid wood unpainted board, with thicknesses ranging from 9mm to 25mm depending on the furniture material used. The specific details are subject to the confirmed drawings of Century Cruise. The environmental protection level of materials must reach E1 level or above.

3.PVC封边条与防火板同纹理及接近颜色，厚度不低于1MM，不脱胶，无空鼓划痕。

3.The PVC edge banding has the same texture and similar color as the fireproof board, with a thickness of not less than 1MM, no delamination, and no hollowing or scratches.

4.五金件采用不锈钢大厂品牌，门合页采用不锈钢通长排铰，抽屉滑轨采用大厂品牌带缓冲。

4. The hardware is made of stainless steel from major manufacturers, the door hinges are made of stainless steel full-length hinges, and the drawer slides are made of stainless steel with buffering from major manufacturers.

5.床板大小与床架一致，安放平整。床架安装牢固，与墙面之间无缝隙，扶手、楼梯方便好用，不松动脱落。

5.The size of the bed board should be consistent with the bed frame and placed flat. The bed frame is firmly installed, with no gaps between it and the wall. The handrails and stairs are convenient and easy to use, without loosening or falling off.

1. 家具台面玻璃，配透明胶垫，玻璃要求钢化并磨边处理。资料柜柜门玻璃为8mm清玻。化妆穿衣镜为6mm厚高清银镜。

6.Furniture countertop glass, equipped with transparent adhesive pads, the glass requires tempering and edging treatment. The door glass of the data cabinet is 8mm clear glass. Makeup and dressing mirror is a 6mm thick high-definition silver mirror.

7.所有焊接口应打磨抛光。

7.All welding joints should be polished and polished.

8.钢架采用正规大厂生产的矩管材料，按照设计厚和表面漆膜要求，但油漆使用水性漆亮光，颜色为浅灰色，以样板色为准。

8.The steel frame is made of rectangular tube material produced by a regular large factory, according to the design thickness and surface paint film requirements, but the paint uses water-based paint with a glossy finish and a light gray color, based on the sample color.

9.所有材料不会出现生锈，腐蚀，生霉，腐烂，起壳，开裂，卷边及开叉等情况。

9.All materials will not experience rusting, corrosion, mold growth, decay, peeling, cracking, curling, or splitting.

10.制造前，制造商需提交深化图纸、每一种饰面材料样板（150mm\*150mm）供世纪游轮审核确认。

10.Before manufacturing, the manufacturer needs to submit detailed drawings and samples of each decorative material (150mm \* 150mm) for Century Cruise's review and confirmation.

11.按照等比例实样的优化需要，尺寸将有所调整。

11.According to the optimization requirements of proportional real samples, the size will be adjusted accordingly.

12.厂商应在批量生产前提交打样样品。

12.Manufacturers should submit sampling samples before mass production.

13.每款产品应保证其稳性。

13.Each product should ensure its stability.

14.产品制造商（销售商）必须确保产品无任何质量问题，并承诺在客户验收一年内对存在问题的所有产品或零件提供免费更换服务，所有产品必须达到合同规定的质量标准，并且适用于商业用途。

14.The product manufacturer (seller) must ensure that the product has no quality problems and promise to provide free replacement services for all products or parts with problems within one year of customer acceptance. All products must meet the quality standards specified in the contract and be suitable for commercial use.