“11码头趸船”装饰工程项目

**PVC地胶手册**

【PVC地胶】

重庆冠达世纪游轮有限公司



**PVC地胶技术说明**

**Poly Vinyl Chloride Technology Explain**

1.产品制造商（销售商）承诺产品质量符合国家标准(GB18586-2001室内装饰装修材料 聚氯乙烯卷材料地板中有害物质)，以及船级社认证相关规范要求（须提供CCS入级船检证书）。

1.The product manufacturer (seller) promises that the product quality meets the national standard (GB18586-2001 Indoor Decoration Materials - PVC Roll Materials - Hazardous Substances in Flooring), as well as the requirements of relevant regulations for classification society certification (CCS classification ship inspection certificate must be provided).

2.安装符合国家建筑装饰质量验收标准《GB5021-2018》。

2.Installation complies with the national building decoration quality acceptance standard GB5021-2018.

3.安装完成后的材料表面图案清晰、色泽一致。

3.After installation, the surface pattern of the material is clear and the color is consistent..

4.材料与基层粘接必须牢固、不空鼓不翘边。

4. The bonding between the material and the base layer must be firm, without hollowing or curling edges.

5.接缝严密无空隙、底胶或焊剂无外溢。与墙边交接处必须吻合，不得显缝。

5.The seams are tight without gaps, and there is no overflow of base glue or solder. The junction with the wall must match and no visible seams are allowed.

6.安装完成后表面需平整、无凹凸不平、无空缺、无翘边、无破损。

6.After installation, the surface should be smooth, without unevenness, gaps, raised edges, or damage.

7.拼花拼色对接处应周边顺畅，走边直线平直，转角处采用对接线拼接，弧形处应符合图纸要求及顺畅美观。

7.The splicing and color matching joints should be smooth around the edges, straight and straight when walking, and the corners should be spliced with matching wires. The curved joints should meet the requirements of the drawings and be smooth and beautiful.

8.清单数据来源于施工图，实际数量以现场最终收方数量为准。

8.The inventory data is sourced from the construction drawings, and the actual quantity is subject to the final quantity received on site.

9.以甲方最终选型封样为准，待甲方确认后才能加工制作。

9.The final selection and sealing sample by Party A shall prevail, and processing and production can only be carried out after confirmation by Party A.

10.制造前，每一种饰面材料样板（300mm\*300mm）或（1219\*149）供世纪游轮审核确认。

10.Before manufacturing, samples of each decorative material (300mm \* 300mm) or (1219 \* 149) shall be provided for Century Cruise's review and confirmation.